
                                              THE USER¡¯S MANUAL OF USB CABLE 

1.Driver Installation:

A.Double click ¡°USB Data Cable Driver ¡° logo of CD-ROM before plug in the cable, and then following the guide step-by-step 
to complete of the installation. 

B.Restart the computer after finish installing. 

C.The computer will download the driver while plugging in the cable. 

2.Notice: connecting the mobile phone (for example: on windows 98 system ) 

A.After plugging in USB Cable, click ¡°my computer / attribute / device management service / port (COM/ LPT) to check whether
there is ¡°USB to Serial Port (COM X ) ¡° or not . The data of ¡°X¡± is different, and probably the computer is different, 
usually the data of ¡°X¡± is superior to ¡®COM 3¡¯. If there isn¡¯t a port like this or this port can not work normally, you
have to confirm the driver installation again. 

B.To install the software which can support your mobile phone and check whether the setup option of communication port from 
the software interface is ¡° USB to Serial Port (COM X)¡±.
(Must confirm this point, otherwise, it is can not connect with your mobile phone) 

C.The best step of using the USB Cable is to plug in USB Cable firstly, then to plug in Mobile Phone and work the software. 
The sequence is opposite while closing. You have to close the software firstly, then pull out USB Cable . Otherwise, the 
computer won¡¯t be work normally or will be cut off.

D.The operation is probably different because the different model of Mobile Phone has different software to support. Moreover
, the software of different model which can support the functions and has the greatest difference. You will be clear the 
detailed information if you check the assistant file of software. 

E.The software, support function and operation way of specific model for USB Cable, and you may check with the dealer. 

3.The below requirements is that the computer connect mobile phone for GPRS: 

A.SIM card has GPRS function (must support by supplier of network in your location);

B.Mobile Phone has GPRS, and support cable transfers. (some model can only support IRDA and MODEM );

C.The correlative software which can support and setup correctly as the software requested. 

D.The different network suppliers of every country has different GPRS APN and setup way. Pls check with the network supplier
for knowing detailed information. 

4.Exception handles: 

A. Plugging in USB Cable to USB port of computer,and checking whether¡°my computer/attribute/device management service/port 
(COM & LPT ) has more COM port . If not, you have to uninstall the driver and install again. 

B. To close the Mobile Phone and re-open it or re-start the computer.

C. Some software possibly did not support the operation system well,such as Window XP.Pls check the software installation 
specification or change operation system testing. 

E.Few computers did not compatible the Driver of USB Cable. Pls change the computer to test.

F.If the above malfunction problems cann¡¯t be solved, pls check with the dealer. 